**PERFORATED LATH ROLLER SHUTTERS**

**SPECIFICATION 3-4**

**Curtain**

Constructed from 76mm curved perforated galvanised steel laths with steel endlocks fitted to alternate laths to prevent lateral movement.

**Bottom Rail**

Galvanised steel inverted “tee” section.

**Guides**

The side guides are formed from galvanised steel channels and prepared for fixing to the opening structure by means of continuous fixing angles.

**Endplates**

Fabricated from mild steel of adequate thickness relative to door size and supplied with angles for fixing to the structure.

**Roller**

The roller is manufactured from mild steel tube of sufficient diameter and wall thickness to resist deflection and is mounted in bearings or cups on each end plate.

**Finish**

The majority of parts are galvanised with other parts prime painted. A polyester powder coated finish in a range of standard RAL colours is available at extra cost.

**Weight**

Approximately 30 kgs per m².

**Operation**

Electrical operation is by means of a single phase tubular motor. A safety brake is fitted to all shutters where personnel could pass underneath thus meeting all relevant Health & Safety requirements. The client should provide a fused spur within 500mm of the motor position.

**Controls**

The standard method of control is by means of internal wall-mounted push buttons.

**Casings**

Coil casings fabricated from galvanised steel sheet are available as an optional extra.

**To specify state:**

**Perforated Lath Roller Shutters shall be by**

**Bolton Gate Company, Waterloo Street, Bolton BL1 2SP, UK Tel: 01204 871001**

**E-mail:** [**sales@boltongate.co.uk**](mailto:sales@boltongate.co.uk) **Web:** [**www.boltongate.co.uk**](http://www.boltongate.co.uk)

**Issue Date: April 2018**