**INSULATED ROLLER SHUTTERS**

**SPECIFICATION 3-8**

**Curtain**

Constructed from 100mm flat galvanised insulated steel laths with endlocks fitted to alternate laths to prevent lateral movement.

**Bottom Rail**

Fabricated from the bottom lath with a galvanised steel trim section and fitted with a rubber weatherstrip.

**Guides**

The side guides are formed from galvanised steel with twin brush strips and prepared for fixing to the opening structure by means of continuous fixing angles.

**Endplates**

Fabricated from mild steel of adequate thickness relative to door size and supplied with angles for fixing to the structure.

**Roller**

The roller is manufactured from mild steel tube of sufficient diameter and wall thickness to resist deflection and is mounted in bearings or cups on each end plate.

**Finish**

Galvanised as standard. A factory finish is available which comprises a white plastisol internal face (coil side) with the external face polyester powder coated to a standard RAL colour.

**Weight**

Approximately 45 kgs per m².

**Operation**

Electrical operation is by means of a direct drive 3 phase geared motor mounted on the outside of one endplate. The motor has an inherent safety brake thus meeting all relevant Health & Safety requirements and the standard unit is pre-wired obviating the need for a site electrician.

**Controls**

The standard method of control is by means of internal wall-mounted push button control. Other types of control including keyswitches etc. are available at extra cost.

**Casings**

Coil casings fabricated from galvanised steel sheet are available as an optional extra.

**To specify state:**

**Insulated Roller Shutters shall be by**

**Bolton Gate Company, Waterloo Street, Bolton BL1 2SP, UK Tel: 01204 871001**

**E-mail:** [**sales@boltongate.co.uk**](mailto:sales@boltongate.co.uk) **Web:** [**www.boltongate.co.uk**](http://www.boltongate.co.uk)

**Issue Date: April 2018**