**EUROFOLD MANUAL FOLDING DOORS**

**SPECIFICATION 1-3**

**Gate Frame**

Constructed from double channel rolled pickets interconnected by galvanised steel lattice bars. Ball bearing pulleys are attached at the top and zinc-plated guide pieces at the bottom.

**Leading Edge**

Galvanised rolled steel section reinforced for handles and locks.

**Leaves**

Formed from 305 x 1.2mm galvanised steel and ribbed for strength. Front hinge strips are attached and the interlocked assembly provides a weather tight installation.

**Top Track**

Galvanised steel rolled section forming a box-type track 90mm deep.

**Bottom Track**

Type B28 galvanised steel “m” section.

**Finish**

The majority of parts are galvanised with other parts prime painted. Polyester powder coating to a range of standard RAL colours is available at extra cost.

**Weight**

Approximately 32 kgs per m².

**Operation**

Manual operation via bow handles attached to each leading edge.

**Locks**

Locking is available via a five-lever deadlock mortised into the leading edge.

**To specify state:**

**Eurofold Manual Folding Doors shall be by**

**Bolton Gate Company, Waterloo Street, Bolton BL1 2SP, UK Tel: 01204 871001**

**E-mail:** [**sales@boltongate.co.uk**](mailto:sales@boltongate.co.uk) **Web:** [**www.boltongate.co.uk**](http://www.boltongate.co.uk)

**Issue Date: April 2018**